{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["技术要求"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"技术要求","index":0,"n_rows":6,"n_cols":5,"rows_kept":6,"merged":[[0,0,0,4],[4,0,4,1],[4,2,4,4],[5,0,5,4]],"flags":["formulas_cached_only"]}
["采购项目清单：可视化移动一键式报警求助系统采购"]
["序号","项目名称","数量或规模","资金预算\n（万元）","资金来源"]
["1、","可视化移动一键式报警求助系统采购","中心院区及妇儿院区护士站、谈话间、医生办公室、收费处、住院处、医患科等约400个点位",47,"自筹"]
["合计",null,null,47]
["备注"]
["技术要求及配置确认书\n一、项目名称、数量：可视化移动一键式报警求助系统采购 ，中心院区及妇儿院区护士站、谈话间、医生办公室、收费处、住院处、医患科等约400个点位可视化移动一键式报警求助系统。                         \n                                                                                               二、项目用途说明：保障医护人员安全，更快有效的处理突发事件。 \n                                                                                              三、配置规格、附件及零配件（包括专用工具）： \n            \n                                                                                                             \n四、详细技术要求、参数及产品资料等：做到与目前安装的有线一键报警连接到一个平台同步管理。提供详细的改造施工方案和后期使用培训方案。提供近三年内与本项目相关类似医院案例。实现两个院区一键报警互联互通。\n可视化移动定位声光报警主机：可视化移动定位报警主机是整个联网报警系统的核心单元，主要用于报警接收处理，支持警灯闪烁提醒、语音播报、视频对接、三维地图联动。\n采用无线报警按钮。支持对报警位置，电池电量，在线状态等信息的实时上报。终端按钮固定式安装，无需布线，可拆式电池，电池可用2年以上。具有小巧美观，且报警无延时功能。\n无线报警网关：一方面接收前端各类传感器和数传终端上传的数据，另一方面将物联数据转换为数据上传至业务处理服务器 。信号传输实现整个院区的覆盖（包括负1层、负2层），支持POE供电。可在接收到一键报警子系统的报警信号后，实现各子系统间的联动；报警时可在地图上自动定位到报警设备，并进行声光提示；报警时联动弹出关联摄像机视频以及周边摄像机视频 ；报警时联动弹出报警处置单；报警时联动弹出处置指导预案、应急通讯录并进行报警信息多维推送。\n提供产品图片及基本参数；提供信息安全服务资质-安全集成资质、信息安全服务资质-安全运维资质和CMM/CMMI能力资质证书；\n\n                                                                                                                                                                                                                                                                                                                \n五、售后服务条件及交货日期（或工期）：售后服务条件：在驻马店市区内有办事处，并且有2人以上的常驻人员。遇有故障半小时内有响应，2小时内解决。"]